%gives the information about the signal data

whos data

%data is the signal data