%plays the given data file

sound(data,fs)

%data is the signal data

%fs is the sample rate